REQUEST FOR PROPOSAL (RFP)
Sewer Ejector Pit Cleaning & Discharge Piping Replacement
Paramus Veterans Memorial Home
New Jersey Department of Veterans Affairs (NJDVA)

1.0 PURPOSE AND INTENT
The New Jersey Department of Veterans Affairs (NJDVA) is soliciting proposals from qualified mechanical contractors to furnish all labor, supervision, materials, equipment, tools, transportation, permits, confined space entry services, testing, and incidentals necessary to perform the complete cleaning of an existing sewer ejector pit and replacement of the sewer ejector discharge piping system at the Paramus Veterans Memorial Home.

The intent of this project is to restore the reliability and operational integrity of the existing sewer ejector system through cleaning of the sewer ejector pit, removal of deteriorated discharge piping and valves, installation of a new discharge piping system, and complete testing and startup of the system.

2.0 SCOPE OF WORK
See the attached Scope of Work 

The Contractor shall provide a complete turnkey installation including, but not limited to:
· Sewer ejector pit cleaning
· Confined space entry
· Wastewater removal and disposal
· Bypass pumping
· Removal of existing piping
· Installation of new discharge piping
· Installation of new check valves
· Installation of new isolation valves
· Pressure and operational testing
· Startup and commissioning

3.0 BIDDER MINIMUM QUALIFICATIONS
The Contractor shall:
a. Possess all licenses required to perform mechanical piping work in the State of New Jersey.
b. Demonstrate experience performing:
· Sewer ejector systems
· Wastewater pumping systems
· Confined space work
· Mechanical piping replacement
c. Be registered with NJSTART.
d. Maintain personnel trained in OSHA Confined Space Entry procedures.

3.1 MANDATORY PRE-BID SITE VISIT
A mandatory site visit shall be conducted prior to bid submission.
The purpose of the site visit is to:
· Verify existing conditions
· Verify dimensions
· Inspect access limitations
· Review piping configuration
· Review confined space requirements
Site visits shall be coordinated through: 
Biko.Hannibal@dva.nj.gov  and William.LeCount@dva.nj.gov

4.0 CONTRACTOR RESPONSIBILITIES
The Contractor shall furnish:
· Labor
· Materials
· Equipment
· Supervision
· Transportation
· Temporary protection
· Testing
· Startup
· Cleanup
· Disposal

The Contractor shall also:
· Verify all field dimensions
· Verify existing piping layout
· Coordinate work with facility personnel
· Protect surrounding equipment and finishes
· Maintain uninterrupted facility operation through bypass pumping
· Restore all disturbed areas

5.0 WORK HOURS
Due to the operational nature of the facility, all work shall be performed during the following hours:
7:00 PM through 5:00 AM
Monday through Friday unless otherwise approved by NJDVA.

6.0 PRICING
Contractors shall provide one lump sum price including:
· Mobilization
· Cleaning
· Bypass pumping
· Confined space entry
· Pipe removal
· Pipe replacement
· Valves
· Testing
· Startup
· Disposal
· Final cleanup
No additional costs will be accepted unless approved through a written NJDVA change order.

7.0 SUBMISSION OF PROPOSALS
Questions shall be submitted by email to:
Biko.Hannibal@dva.nj.gov  and William.LeCount@dva.nj.gov

Subject:
Sewer Ejector Pit RFP
Questions shall be received no later than: July 10, 2026

Email proposals to:
Biko.Hannibal@dva.nj.gov  and William.LeCount@dva.nj.gov

Subject:
Bid Proposal – Sewer Ejector Pit Cleaning & Discharge Piping Replacement
Proposal Due Date: July 17, 2026


8.0 PROJECT LOCATION
Paramus Veterans Memorial Home
1 Veterans Drive
Paramus, NJ 07652

9.0 INSURANCE
The Contractor shall maintain insurance meeting State of New Jersey requirements.

10.0 PERMITS
The Contractor shall obtain all permits required.



